{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":145,"n_cols":9,"rows_kept":145,"merged":[[0,0,0,8],[1,0,1,8],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,2,4],[2,7,3,7],[2,8,3,8],[4,0,14,0],[4,1,14,1],[4,4,14,4],[4,5,14,5],[4,6,14,6],[4,8,14,8],[7,3,14,3],[15,0,29,0],[15,1,25,1],[15,3,17,3],[15,4,24,4],[15,5,17,5],[15,6,17,6],[15,8,25,8],[18,3,25,3],[18,5,24,5],[18,6,29,6],[26,1,29,1],[26,3,29,3],[26,4,29,4],[26,5,29,5],[26,8,28,8],[30,0,31,0],[30,1,31,1],[30,4,31,4],[30,5,31,5],[30,6,31,6],[30,8,31,8],[32,0,44,0],[32,1,44,1],[32,3,44,3],[32,4,44,4],[32,5,44,5],[32,6,44,6],[45,0,58,0],[45,1,52,1],[45,3,58,3],[45,4,58,4],[45,5,58,5],[45,6,58,6],[45,8,52,8],[53,1,56,1],[53,2,56,2],[53,7,56,7],[57,1,58,1],[57,8,58,8],[59,0,70,0],[59,1,70,1],[59,3,70,3],[59,4,70,4],[59,5,70,5],[59,6,70,6],[59,8,63,8],[64,8,69,8],[72,0,83,0],[72,1,74,1],[72,3,83,3],[72,4,83,4],[72,8,77,8],[75,1,78,1],[79,1,83,1],[79,8,81,8],[84,0,88,0],[84,1,88,1],[84,3,88,3],[84,4,88,4],[85,8,87,8],[89,0,92,0],[89,2,92,2],[89,3,92,3],[89,4,92,4],[89,6,92,6],[89,7,92,7],[89,8,92,8],[93,0,102,0],[93,1,102,1],[93,3,96,3],[93,4,106,4],[97,3,102,3],[97,8,100,8],[103,0,104,0],[103,1,104,1],[103,8,104,8],[105,0,106,0],[105,1,106,1],[105,3,106,3],[105,8,106,8],[107,0,136,0],[107,1,136,1],[107,3,136,3],[107,4,136,4],[107,8,135,8],[137,0,144,0],[137,1,144,1],[137,3,144,3],[137,4,144,4],[137,8,144,8]]}
["华新环境工程（武穴）有限公司"]
["日常监测计划一览表"]
["项目","监测位置","检测类别","监测频率",null,"监测","监测","排放标准","执行标准"]
[{"$nulls":3},"自测","委托监测","时间","单位"]
["废水（地表水）","污水处理站进、出口，主要处理单元出口","COD","在线检","一年4次","3、6、9、12月各一次","委托第三方监测机构","500mg/L","《污水综合排放标准》（GB8978-1996)表4三级标准、表1标准"]
[null,null,"氨氮","测设备",{"$nulls":3},"/"]
[null,null,"PH",{"$nulls":4},"6—9"]
[null,null,"BOD5",{"$nulls":4},"300mg/L"]
[null,null,"悬浮物",{"$nulls":4},"400mg/L"]
[null,null,"磷酸盐",{"$nulls":4},"/"]
[null,null,"LAS",{"$nulls":4},"20mg/L"]
[null,null,"石油类",{"$nulls":4},"20mg/L"]
[null,null,"砷",{"$nulls":4},"0.5mg/L"]
[null,null,"镉",{"$nulls":4},"0.1mg/L"]
[null,null,"铅",{"$nulls":4},"1.0mg/L"]
["废气","窑尾","颗粒物","在线监测设备","一季度一次","/","/","30mg/m3","《水泥工业大气污染物排放标准（GB4915-2013）》表1、《水泥窑协同处置固体废物污染控制标准（GB30485-2013）》表1"]
[null,null,"二氧化硫",{"$nulls":4},"200mg/m3"]
[null,null,"氮氧化物（以 NO2计）",{"$nulls":4},"400mg/m3"]
[null,null,"总有机碳","/",null,"/","委托第三方监测机构","120mg/m3"]
[null,null,"氟化物",{"$nulls":4},"5mg/m3"]
[null,null,"氯化氢",{"$nulls":4},"10mg/m3"]
[null,null,"氟化氢",{"$nulls":4},"1mg/m3"]
[null,null,"汞及其化合物（以Hg计）",{"$nulls":4},"0.05mg/m3"]
[null,null,"铊、镉、铅、砷及其化合物（以Tl+Cd+Pb+AS计）",{"$nulls":4},"1.0mg/m3"]
[null,null,"铍、铬、锡、锑、铜、钴、锰、镍、钒及其化合物（以Be+Cr+Sn+Sb+Cu+Co+Mn+Ni+V计）",{"$nulls":4},"0.5mg/m3"]
[null,null,"二噁英类(毒性当量)",null,"一年一次","/",null,"0.1ng TEQ/m3"]
[null,"厂界（至少4个点）","臭气浓度",null,"一季度一次","3、6、9、12月各一次",null,"20mg/m3","《恶臭污染物排放标准》（GB14554-93）表1 "]
[null,null,"氨",{"$nulls":4},"1.5mg/m3"]
[null,null,"硫化氢",{"$nulls":4},"0.06mg/m3"]
[null,null,"颗粒物(粉尘)",{"$nulls":4},"1.0mg/m3","GB16297-1996《大气污染物综合排放标准》"]
["噪声","厂界外1米， 4个监测点","昼间",null,"一年四次","3、6、9、12月各一次","委托第三方监测机构",65,"《工业企业厂界环境噪声排放标准》（GB 12348-2008）3类"]
[null,null,"夜间",{"$nulls":4},55]
["地下水","地下水（4个监测点位）","pH ","/","每季度一次","3、6、9、12月各一次","委托第三方监测机构","6.5～8.5","《地下水质量标准》(GB/T 14848-2017）表1"]
[null,null,"总硬度",{"$nulls":4},"450mg/L","3类标准"]
[null,null,"总大肠菌数",{"$nulls":4},"3个/L"]
[null,null,"高锰酸盐指数",{"$nulls":4},"3.0mg/L"]
[null,null,"氨氮",{"$nulls":4},"0.5mg/L"]
[null,null,"氯化物",{"$nulls":4},"250mg/L"]
[null,null,"氰化物",{"$nulls":4},"0.05mg/L"]
[null,null,"总砷",{"$nulls":4},"0.05mg/L"]
[null,null,"总汞",{"$nulls":4},"0.001mg/L"]
[null,null,"氟化物",{"$nulls":4},"1.0mg/L"]
[null,null,"总铅",{"$nulls":4},"0.05mg/L"]
[null,null,"总镍",{"$nulls":4},"0.05mg/L"]
[null,null,"总铬（六价）",{"$nulls":4},"0.05mg/L"]
["土壤","厂区内","铜","/","每年一次","/","委托第三方监测机构","400mg/kg","《土壤环境质量标准》（GB15618-1995)表1 三级标准"]
[null,null,"锌",{"$nulls":4},"500mg/kg"]
[null,null,"铅",{"$nulls":4},"500mg/kg"]
[null,null,"镉",{"$nulls":4},"1.0mg/kg"]
[null,null,"总砷",{"$nulls":4},"40mg/kg"]
[null,null,"总汞",{"$nulls":4},"1.5mg/kg"]
[null,null,"总铬",{"$nulls":4},"300mg/kg"]
[null,null,"镍",{"$nulls":4},"200mg/kg"]
[null,"厂址外污染土堆棚西北侧","二噁英",{"$nulls":4},"4000pg TEQ/kg","参考标准：（按最严执行）"]
[{"$nulls":8},"德国5000pg/kg"]
[{"$nulls":8},"加拿大4000pg/kg"]
[{"$nulls":8},"日本1000ng/kg"]
[]
[]
["环境","人口稠密区和敏感点（2-3个点）","SO2","/","一年一次","/","委托第三方监测机构","0.06mg/m3","GB3095-1996 及其修改单二级标准"]
[null,null,"NO2",{"$nulls":4},"0.08 mg/m3"]
[null,null,"TSP",{"$nulls":4},"0.20 mg/m3"]
[null,null,"Pb",{"$nulls":4},"1.00 mg/m3"]
[null,null,"氟化物（F）",{"$nulls":4},"20 mg/m3"]
[null,null,"氯化氢（HCl）",{"$nulls":4},"0.05 mg/m3","TJ36-79"]
[null,null,"NH3",{"$nulls":4},"0.20 mg/m3"]
[null,null,"H2S",{"$nulls":4},"0.01 mg/m3"]
[null,null,"Hg",{"$nulls":4},"0.0003 mg/m3"]
[null,null,"砷化物（As）",{"$nulls":4},"0.003 mg/m3"]
[null,null,"锰及其化合物",{"$nulls":4},"0.01 mg/m3"]
[null,null,"二噁英",{"$nulls":4},"0.6pg TEQ/m3","湖北省环保厅复函：鄂环函[2011]1087 号"]
["类别","监测点","污染因子/监测因子","自测","委托监测",null,"备注","标准限值","执行排放标准名称"]
["有组织废气","除臭楼排放口","氨",null,"一季度一次",null,null,"35kg/h","恶臭污染物排放标准GB14554-93"]
[null,null,"硫化氢",{"$nulls":4},"2.3 kg/h"]
[null,null,"臭气浓度",{"$nulls":4},20000]
[null,"危废储存废气排放口","氨",{"$nulls":4},"4.9 kg/h"]
[null,null,"硫化氢",{"$nulls":4},"0.33 kg/h"]
[null,null,"臭气浓度",{"$nulls":4},2000]
[null,null,"挥发性有机物",{"$nulls":4},"80mg/m3","工业企业挥发性有机物排放控制标准》（DB12/524-2014）"]
[null,"危废预处理排放口","氨",{"$nulls":4},"14 kg/h","恶臭污染物排放标准GB14554-93"]
[null,null,"硫化氢",{"$nulls":4},"0.9 kg/h"]
[null,null,"臭气浓度",{"$nulls":4},6000]
[null,null,"挥发性有机物",{"$nulls":4},"80mg/m3","工业企业挥发性有机物排放控制标准》（DB12/524-2014）"]
[null,null,"颗粒物",{"$nulls":4},"20mg/m3","《水泥工业大气污染物排放标准》"]
["无组织废气","厂界上风向一个，下风向3个","颗粒物",null,"一季度一次",null,null,"0.5mg/Nm3","大气污染物综合排放标准GB16297-1996"]
[null,null,"氨",{"$nulls":4},"1.5 mg/Nm3","恶臭污染物排放标准GB14554-93"]
[null,null,"硫化氢",{"$nulls":4},"0.06 mg/Nm3"]
[null,null,"臭气浓度",{"$nulls":4},20]
[null,null,"挥发性有机物",{"$nulls":3},"1h平均浓度值","10 mg/Nm3","挥发性有机物无组织排放控制标准GB 37822-2019"]
["噪声","项目厂界东侧外1m处","等效连续A声级",null,"一季度一次",null,null,"昼间≤65dB(A)，夜间≤55dB(A)","GB 12348-2008 工业企业厂界环境噪声排放标准"]
[null,"项目厂界南侧外1m处"]
[null,"项目厂界西侧外1m处"]
[null,"项目厂界北侧外1m处"]
["废水","污水处理站排放口","pH值","在线监测设备","一月一次",null,null,"2022-06-09","污水综合排放标GB8978-1996"]
[null,null,"悬浮物",{"$nulls":4},"250mg/L","排水协议"]
[null,null,"五日生化需氧量",{"$nulls":4},"200 mg/L","排水协议"]
[null,null,"化学需氧量",{"$nulls":4},"410 mg/L","排水协议"]
[null,null,"总汞",{"$nulls":4},"0.05 mg/L","污水综合排放标GB8978-1996"]
[null,null,"总镉",{"$nulls":4},"0.1 mg/L"]
[null,null,"总砷",{"$nulls":4},"0.5 mg/L"]
[null,null,"总铅",{"$nulls":4},"1.0mg/L"]
[null,null,"氨氮（NH3-N）",{"$nulls":4},"41 mg/L","排水协议"]
[null,null,"总磷（以P计）",{"$nulls":4},"7.5 mg/L","排水协议"]
["雨水","雨水排放口","化学需氧量",{"$nulls":4},"500mg/L","污水综合排放标GB8978-1996"]
[null,null,"悬浮物",{"$nulls":4},"400mg/L"]
["雨水","雨水排放口","悬浮物",{"$nulls":4},"70mg/L","污水综合排放标GB8978-1996"]
[null,null,"化学需氧量",{"$nulls":4},"100 mg/L"]
["地下水","地下水监测井","pH值",null,"一年三次，枯、平、丰各一次。",null,null,"6.5-8.5","地下水质量标准（GB/T14848-2017）"]
[null,null,"色度",{"$nulls":4},15]
[null,null,"浑浊度",{"$nulls":4},"3NTU"]
[null,null,"溶解性总固体",{"$nulls":4},"1000mg/L"]
[null,null,"总硬度",{"$nulls":4},"450 mg/L"]
[null,null,"高锰酸盐指数",{"$nulls":4},"3.0 mg/L"]
[null,null,"总大肠菌群",{"$nulls":4},"3.0MPN/100mL"]
[null,null,"阴离子表面活性剂",{"$nulls":4},"0.3 mg/L"]
[null,null,"总汞",{"$nulls":4},"0.001 mg/L"]
[null,null,"总镉",{"$nulls":4},"0.005 mg/L"]
[null,null,"六价铬",{"$nulls":4},"0.05 mg/L"]
[null,null,"总砷",{"$nulls":4},"0.01 mg/L"]
[null,null,"总铅",{"$nulls":4},"0.01 mg/L"]
[null,null,"总镍",{"$nulls":4},"0.02 mg/L"]
[null,null,"总铜",{"$nulls":4},"1.00 mg/L"]
[null,null,"总锌",{"$nulls":4},"1.00 mg/L"]
[null,null,"总锰",{"$nulls":4},"0.10 mg/L"]
[null,null,"总铁",{"$nulls":4},"0.3 mg/L"]
[null,null,"总硒",{"$nulls":4},"0.01 mg/L"]
[null,null,"氨氮（NH3-N）",{"$nulls":4},"0.50 mg/L"]
[null,null,"亚硝酸盐",{"$nulls":4},"1.00 mg/L"]
[null,null,"硝酸盐（以N计）",{"$nulls":4},"20.0 mg/L"]
[null,null,"氰化物",{"$nulls":4},"0.05 mg/L"]
[null,null,"氟化物（以F-计）",{"$nulls":4},"1.0 mg/L"]
[null,null,"氯化物（以Cl-计）",{"$nulls":4},"250 mg/L"]
[null,null,"硫酸盐（以SO42-计）",{"$nulls":4},"250 mg/L"]
[null,null,"挥发酚",{"$nulls":4},"0.002 mg/L"]
[null,null,"苯",{"$nulls":4},"10.0 ug/mL"]
[null,null,"甲苯",{"$nulls":4},"700ug/mL"]
[null,null,"石油类",{"$nulls":4},"0.05mg/L","地表水质量标准（GB3838-2002）"]
["土壤","土壤监测点","总汞",null,"一季度一次",null,null,"38mg/kg","《土壤环境质量标准—建设用地土壤污染风险管控标准》（GB36600-2018）"]
[null,null,"总镉",{"$nulls":4},"65 mg/kg"]
[null,null,"六价铬",{"$nulls":4},"5.7 mg/kg"]
[null,null,"总砷",{"$nulls":4},"60 mg/kg"]
[null,null,"总铅",{"$nulls":4},"800 mg/kg"]
[null,null,"总镍",{"$nulls":4},"900 mg/kg"]
[null,null,"总铜",{"$nulls":4},"18000 mg/kg"]
[null,null,"二噁英",{"$nulls":4},"4×10-5mg/kg(40ng-TEQ/k)"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}